xRANc-SouthBound-API

Table of Contents

[2 Introduction 2](#_Toc486603665)

[3 Message Description 3](#_Toc486603666)

[3.1 Transport Layer 3](#_Toc486603667)

[3.2 Configuration Messages 3](#_Toc486603668)

[3.2.1 XRANC\_CELL\_CONFIG 3](#_Toc486603669)

[3.2.2 UE Capability 7](#_Toc486603670)

[3.3 Procedural Messages 8](#_Toc486603671)

[3.3.1 UE\_ADMISSION\_CONTROL 8](#_Toc486603672)

[3.3.2 HANDOFF 10](#_Toc486603673)

[3.3.3 XRANC\_BEARER\_MANAGEMENT 12](#_Toc486603674)

[3.4 Measurements 16](#_Toc486603675)

[3.4.1 EUTRAN Periodic Measurements 16](#_Toc486603676)

[3.4.2 L2 Measurements 17](#_Toc486603677)

[3.5 xICIC/Coordinated Scheduling Controls 23](#_Toc486603678)

[3.6 Carrier Aggregation Controls 24](#_Toc486603679)

Figure 1: Basic xRAN Architecture 2

Figure 2: Cell-configuration 3

Figure 3: UE Capability Information Exchange 7

Figure 4: UE Admission Control 8

Figure 5: Handoff 11

Figure 6: Bearer Admission and Modification 13

Figure 7: EUTRAN Periodic Measurements 16

Figure 8: L2 Measurements 17

Figure 9: ICIC Controls 23

Figure 10: Carrier Aggregation Control 25

# Introduction

xRANc-AP

xRANc-AP

Control plane application

xRAN controller

xRANc-API

xRANc-API

xRAN Agent

Sch

L1/2/3

xRAN Agent

Sch

L1/2/3

Figure 1: Basic xRAN Architecture

The xRAN controller implements the control plane functionality interfacing with the eNodeB data-plane functionality through the xRANc-API. The control plane functionality will include, but is not limited to, UE Admission Control, Radio Bearer Admission and Modification, Handoffs, and Load Balancing, Inter-cell Interference Coordination etc.

# Message Description

## Transport Layer

The transport layer for the xRANc-API will be SCTP. It will be assumed that the topology information, along with the ECGI for each cells with corresponding IP/Port for the SCTP connection is available at the xran-controller aprior. The value 0 will be used for the SCTP payload protocol identifier.

## Configuration Messages

### XRANC\_CELL\_CONFIG

On initiation, the xranc will send periodic CELL\_CONFIG\_REQUEST messages to the eNodeB, until it receives a response from the cells. The eNodeB will respond back with CELL\_CONFIG\_REPORT message. On receiving this response, the xranc will assume that the cell is up and running, and is under the purview of the xranc.

The xranc may send CELL\_CONFIG\_REQUEST messages periodically to check or get updates on the cell configuration.

In future, the API will be expanded to allow the xran-controller the ability to configure these messages as well as for the eNodeB to send the config report uninitiated, by the xran controller.

**eNodeB**

**xRANc**

CELL\_CONFIG\_REQUEST

CELL\_CONFIG\_REPORT

Figure 2: Cell-configuration

**CELL\_CONFIG\_REQUEST**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Values | Description |
| ecgi | ECGI | E-UTRAN Global Cell ID (PLMN ID + ENodeB ID + Cell ID) |

**ECGI**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Values | Description |
| PLMN-Identity | OCTET STRING (SIZE(3)) | PLMN identity - digits 0 to 9, encoded 0000 to 1001, - 1111 used as filler digit, two digits per octet, - bits 4 to 1 of octet n encoding digit 2n-1 - bits 8 to 5 of octet n encoding digit 2n -The Selected PLMN identity consists of 3 digits from MCC followed by either -a filler digit plus 2 digits from MNC (in case of 2 digit MNC) or -3 digits from MNC (in case of a 3 digit MNC). |
| EUTRANCellIdentifier | BIT STRING (SIZE (28)) |  |

**CELL\_CONFIG\_REPORT**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Values | Description |
| ecgi | ECGI | E-UTRAN Global Cell ID (PLMN ID + ENodeB ID + Cell ID) |
| pci | PhysCellId | Physical Cell Identity |
| candidate\_scells | SEQUENCE OF CandScell | PCI and Downlink EARFCN of the cells that can be configured as secondary cell with this cell’s primary component carrier |
| earfcn\_dl | ARFCN-Value | Downlink EARFCN |
| earfcn\_ul | ARFCN-Value | Uplink EARFCN |
| rbs\_per\_tti\_dl | INTEGER | Downlink Bandwidth (in RBs per TTI) |
| rbs\_per\_tti\_ul | INTEGER | Uplink Bandwidth (in RBs per TTI) |
| num\_tx\_antenna | INTEGER | Number of TX Antenna ports |
| duplex\_mode | ENUMERATED(fdd,tdd) | TDD(1) or FDD(0) |
| tdd\_config | INTEGER(0..6) OPTIONAL | TDD Uplink-Downlink config |
| tdd\_Spl\_sf\_config | INTEGER(0..8) OPTIONAL | TDD Special Subframe config |
| max\_num\_connected\_ues | INTEGER | Maximum number of UEs in RRC\_Connected State that the cell can support |
| max\_num\_bearers | INTEGER | Maximum number of bearers that the cell can support |
| max\_num\_ues\_sched\_per\_tti\_dl | INTEGER | Max number of UEs that can be scheduled for TX per TTI in the Downlink |
| max\_num\_ues\_sched\_per\_tti\_ul | INTEGER | Max number of UEs that can be scheduled for TX per TTI in the Uplink |
| dlfs\_sched\_enable | BOOLEAN | Sched does Frequency Selective Scheduling in the DL |

**CandScell**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Values | Description |
| pci | PhysCellId | Physical Cell Identity |
| earfcn-dl | ARFCN-Value | downlink EARFCN |

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Values | Description |
| PhysCellId | INTEGER (0..503) |  |
| ARFCN-Value | INTEGER (0..65535) |  |

### UE Capability

Upon receiving UECapabilityEnquiry from xRANc, the eNB obtains the UE capabilities (if not already) and responds with UECapabilityInfo.



Figure 3: UE Capability Information Exchange

**UECapabilityEnquiry**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Values | Description |
| crnti | CRNTI | C-RNTI assigned to UE |
| ecgi | ECGI | Global cell Id of connecting cell |

**UECapabilityInfo**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Values | Description |
| crnti | CRNTI | C-RNTI assigned to UE |
| ecgi | ECGI | Global cell Id of connecting cell |
| ca-cap | CACap | Capabilities related to CA |

**CACap**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Values | Description |
| band | INTEGER | C-RNTI assigned to UE |
| caclassdl | ENUMERATED(a,b,c,d,e,f,…) | DL capabilities related to CA |
| caclassul | ENUMERATED(a,b,c,d,e,f,…) | DL capabilities related to CA |
| crossCarrierSched | BOOLEAN | True if supported by the UE, else False |

## Procedural Messages

### UE\_ADMISSION\_CONTROL



Figure 4: UE Admission Control

**UE\_ADMISSION\_REQUEST**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Values | Description |
| crnti | CRNTI | C-RNTI assigned to UE |
| ecgi | ECGI | Global cell Id of connecting cell |
| adm\_est\_cause | ENUMERATED (emergency, highp-access, mt-access, mo-signalling,mo-data) | Connection establishment cause |

**UE\_ADMISSION\_RESPONSE**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| crnti | CRNTI | C-RNTI assigned to UE |
| ecgi | ECGI | Cell Id of connecting cell |
| adm\_est\_response | ENUMERATED(success, failure) | Success of Failure; Cause value if failure (TBD) |

**UE\_ADMISSION\_STATUS**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| crnti | CRNTI | C-RNTI assigned to UE |
| ecgi | ECGI | Cell Id of connecting cell |
| adm\_est\_status | ENUMERATED(success, failure) | Success or Failure; Cause value if Failure |

**UE\_CONTEXT\_UPDATE**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| crnti | CRNTI | C-RNTI assigned to UE |
| ecgi | ECGI | Cell Id of connecting cell |
| mme\_ue\_s1ap\_id | MME-UE-S1AP-ID | ID for UE association over the S1 interface within the MME |
| enb\_ue\_s1ap\_id | ENB-UE-S1AP-ID | ID for UE association over the S1 interface within the eNB |

**UE\_RECONFIG\_IND**

(sent from eNodeB to xRAN controller, on RRC Connection Re-Establishment complete)

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| crnti\_old | CRNTI | Old C-RNTI assigned to UE |
| ecgi | ECGI | Cell Id of connecting cell |
| crnti\_new | CRNTI | New C-RNTI assigned to UE |
| reconfig\_cause | ENUMERATED (rlf, ho-fail, others) | Cause value for Reconfig |

**UE\_RELEASE\_IND**

(eNodeB -> xRANc is indication when UE goes from RRC\_ACTIVE to RRC\_IDLE, and xRANc -> eNodeB is control when xRANc wants to deactivate the UE)

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| crnti | CRNTI | Old C-RNTI assigned to UE |
| ecgi | ECGI | Cell Id of connecting cell |
| release\_cause | ENUMERATED (inactivity, rlf, others) | releaseCause |

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Values | Description |
| CRNTI | BIT STRING (SIZE (16)) |  |
| MME-UE-S1AP-ID | INTEGER (0..4294967295) |  |
| ENB-UE-S1AP-ID | INTEGER (0..16777215) |  |

### HANDOFF



Figure 5: Handoff

**HANDOFF\_REQUEST**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| crnti | CRNTI | C-RNTI assigned to UE |
| ecgi\_s | ECGI | Cell ID of source cell |
| ecgi\_t | ECGI | Cell ID of target cell |

*Note: The xRAN controller sends the “HO request”message to both the Source and Target eNodeB. This way, the target eNodeB also is informed to expect an X2/S1 handover message from the source eNodeB. If the X2 interface does not exist between the source and the target eNode, the eNodeBs can do a S1 based HO.*

**HANDOFF\_FAILURE**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| crnti | CRNTI | C-RNTI assigned to UE |
| ecgi\_s | ECGI | Cell ID of source cell |
| ho\_failure\_cause | ENUMERATED (other) | Cause for failure (TBD) |

*Note: If the source eNodeB gets a negative response from the target eNodeB as part of the “X2AP:Handover request ack”, then the source eNodeB sends the HO failure message to the eNodeB. If noth, then the source eNodeB sends a “RRC Connection Reconfig” message to the eNodeB.*

**HANDOFF\_COMPLETE**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| crnti\_new | CRNTI | New c-RNTI assigned to the UE by the Target eNodeB |
| ecgi\_s | ECGI | Global Cell ID of source cell |
| ecgi\_t | ECGI | Global Cell ID of the target cell |

*Note: Sent to the xRAN controller, on receiving the “RRC Connection Reconfig” message by the target eNodeB.*

### XRANC\_BEARER\_MANAGEMENT

**eNodeB**

**xRANc**

Bearer

Admission Control

**XRANC\_BEARER\_ADMISSION\_STATUS**

**XRANC\_BEARER\_ADMISSION\_RESPONSE**

**XRANC\_BEARER\_ADMISSION\_REQUEST**

Figure 6: Bearer Admission and Modification

**XRANC\_BEARER\_ADMISSION\_REQUEST**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| crnti | CRNTI | C-RNTI assigned to UE |
| ecgi | ECGI | Global Cell ID |
| ue\_ambr | UEAMBR | [UE AMBR DL, UE AMBL UL] |
| num\_erabs\_list | INTEGER(1..maxNumERABS) | Number of eRABS to be added or modified |
| erabs\_params | SEQUENCE (SIZE (1..maxNumERABS)) OF ERABParams-Item | List of ERABs to be added or modified with bearer\_params |

**XRANC\_BEARER\_ADMISSION\_RESPONSE**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| crnti | CRNTI | C-RNTI assigned to UE |
| ecgi | ECGI | Global Cell ID |
| num\_erab\_list | INTEGER(1..maxNumERABS) | Number of eRABS to be added or modified |
| erabs\_status | SEQUENCE (SIZE (1..maxNumERABS)) OF ERABResponse-Item | Success or Failure (List of Causes) |

**XRANC\_BEARER\_ADMISSION\_STATUS**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| crnti | CRNTI | C-RNTI assigned to UE |
| ecgi | ECGI | Global Cell ID |
| num\_erab\_list | INTEGER(1..maxNumERABS) | Number of eRABS to be added or modified |
| erabs\_status | SEQUENCE (SIZE (1..maxNumERABS)) OF ERABResponse-Item | Success or Failure (List of Causes) |

**XRANC\_BEARER\_RELEASE\_IND**

**(From eNodeB to xRANc)**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| crnti | CRNTI | C-RNTI assigned to UE |
| ecgi | ECGI | Global Cell ID |
| num\_erab\_list | INTEGER(1..maxNumERABS) | Number of eRABS to be added or modified |
| erabs\_ids | SEQUENCE (SIZE (1..maxNumERABS) ) OF ERAB-ID | List of erabs released |

**UEAMBR**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| ambr-dl | BitRate |  |
| ambr-ul | BitRate |  |

**ERABParams-Item**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| id | ERAB-ID |  |
| direction | ERABDirection |  |
| type | ERABtype |  |
| qci | QCI |  |
| arp | INTEGER |  |
| gbr-dl | BitRate |  |
| gbr-ul | BitRate |  |
| mbr-dl | BitRate |  |
| mbr-ul | BitRate |  |

**ERABResponse-Item**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| id | ERAB-ID |  |
| decision | ERABDecision |  |

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| BitRate | INTEGER (0..10000000000) |  |
| ERAB-ID | INTEGER (0..15, ...) |  |
| ERABDirection | ENUMERATED (dl, ul, both) |  |
| ERABType | ENUMERATED (default, dedicated) |  |
| QCI | INTEGER (0..255) |  |
| maxNumERABS | INTEGER ::= 11 | constant |

## Measurements

### EUTRAN Periodic Measurements

**eNodeB**

**UE**

**xRANc**

XRANC\_RS\_SIGNAL\_MEAS\_REPORT

XRANC\_RX\_SIGNAL\_MEAS\_CONFIG

RRC connection

reconfig

(meas. Config)

(

RRC meas. report

(periodic)

Figure 7: EUTRAN Periodic Measurements

**XRANC\_RX\_SIGNAL\_MEAS\_CONFIG**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| ecgi | ECGI | Cell ID of associated cell |
| crnti | CRNTI | CRNTI of UE |
| report\_qty | ENUMERATED (RSRP = 0, RSRQ = 1, BOTH = 2) | RSRP/RSRQ/BOTH |
| meas\_cells | SEQUENCE OF PCI-ARFCN | PCI and downlink EARFCN of the cells to perform measurement on |
| report\_interval\_ms | ENUMERATED (ms-120, ms-240, ms-480,ms-640, ms-1024, ms-2048, ms-5120, ms-10240, min-1, min-6, min-12, min-30, min-60) | Time between sending two measurement reports |

**XRANC\_RX\_SIGNAL\_MEAS\_REPORT**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| crnti | CRNTI | CRNTI of UE |
| ecgi | ECGI | Cellid of associated cell |
| cell\_meas\_reports | SEQUENCE OF RXSigReport | RSRP/RSRQ of cells on which measurement is performed |

**RXSigReport**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| pci-arfcn | PCI-ARFCN |  |
| rsrp | RSRP-Range |  |
| rsrq | RSRQ-Range |  |

**PCI-ARFCN**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Values | Description |
| pci | PhysCellId | Physical Cell Identity |
| earfcn-dl | ARFCN-Value | Downlink EARFCN |

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| RSRP-Range | INTEGER(0..97) |  |
| RSRQ-Range | INTEGER(0..34) |  |

### L2 Measurements

**eNodeB**

**xRANc**

XRANC\_L2\_MEAS\_CONFIG

L2 Measurement

Reports

(periodic)

Figure 8: L2 Measurements

**XRANC\_L2\_MEAS\_CONFIG**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| eCGI | ECGI | Cell ID of associated cell |
| report\_interval\_ms | INTEGER | Time between sending two measurement reports (T)  (min time – 100ms) |

**Note: For all L2 measurements, to support partial features, an invalid measurement value can be indicated by reporting 0xFFFF for that field.**

**XRANC\_RADIO\_MEAS\_REPORT\_PER\_UE**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| ecgi | ECGI | Cell ID of associated cell |
| crnti | CRNTI | CRNTI of UE |
| radio\_report\_serv\_cells | SEQUENCE OF RadioRepPerServCell | Radio report over the set of serving cells |

**RadioRepPerServCell**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| pci-arfcn | PCI-ARFCN |  |
| cqi\_hist | SEQUENCE (SIZE(maxNumCQIs)) OF INTEGER | CQI distribution reported by each UE over the measurement period (configured by xRANc) |
| ri\_hist | SEQUENCE (SIZE(maxNumRIs)) OF INTEGER | Number of rank 1 and rank 2 samples as reported by the UE over the measurement period (configured by xRANc) |
| pusch\_sinr\_hist | SEQUENCE (SIZE(sinrHistSize)) OF INTEGER | PUSCH SINR distribution measured by the eNodeB for the UE in ranges (-inf,-18], (-18,-15], (-15,-12], (-12,-9], (-9,-6], (-6,-3], (-3,-0], (-0,3], (3,6], (6,9], (9,12], (12,15], (15,18], (18,inf)} |
| pucch\_sinr\_hist | SEQUENCE (SIZE(sinrHistSize)) OF INTEGER | PUCCH SINR distribution measured by the eNodeB for the UE in ranges { (-inf,-18], (-18,-15], (-15,-12], (-12,-9], (-9,-6], (-6,-3], (-3,0], (0,3], (3,6], (6,9], (9,12], (12,15], (15,18], (18,inf)} |

**XRANC\_RADIO\_MEAS\_REPORT\_PER\_CELL**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| ecgi | ECGI | Cell ID of associated cell |
| pusch\_intf\_pwr\_hist | SEQUENCE (SIZE(intrfHistSize)) OF INTEGER | PUSCH interference + noise power (dBm) distribution measured by the eNodeB on the uplink in ranges {(-inf,-120], (-120,-118], (-118,-116], (-116,-114], (-114,-112], (-112,-110], (-110,-108], (-108,-106], (-106,-104], (-104,-102], (-102,-100], (-100,-98], (-98,-96], (-96,-94], (-94,-92], (-92,-90], (-90,inf)} |
| pucch\_intf\_power\_hist | SEQUENCE (SIZE(intrfHistSize)) OF INTEGER | PUCCH interference + noise power (dBm) distribution measured by the eNodeB on the uplink in ranges {(-inf,-120], (-120,-118], (-118,-116], (-116,-114], (-114,-112], (-112,-110], (-110,-108], (-108,-106], (-106,-104], (-104,-102], (-102,-100], (-100,-98], (-98,-96], (-96,-94], (-94,-92], (-92,-90], (-90,inf)} |

**XRANC\_SCHED\_MEAS\_REPORT\_PER\_UE**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| ecgi | ECGI | Cell ID of associated cell |
| crnti | CRNTI | CRNTI of UE |
| sched-report-serv-cells | SEQUENCE OF SchedMeasRepPerServCell | scheduler report over the set of serving cells |

**SchedMeasRepPerServCell**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| pci-arfcn | PCI-ARFCN |  |
| qci\_vals | SEQUENCE (SIZE(1..maxNumSupQCI)) OF QCI | QCI values for which the following information is reported |
| prb\_usage | PRBUsage | Percentage of PRBs allocated to this CRNTI in downlink and uplink |
| mcs\_dl | SEQUENCE (SIZE(1..maxNumSupQCI)) OF INTEGER | DL MCS per UE per QCI, where each element is the average of the MCS allocated for that QCI for that UE over the time period |
| num\_sched\_ttis\_dl | SEQUENCE (SIZE(1..maxNumSupQCI)) OF INTEGER | DL Scheduled time per UE per QCI, i.e., total TTIs where that UE was scheduled on the DL for that QCI |
| mcs\_ul | SEQUENCE (SIZE(1..maxNumSupQCI)) OF INTEGER | UL MCS per UE per QCI, where each element is the average of the MCS allocated for that QCI for that UE over the time period |
| num\_sched\_ttis\_ul | SEQUENCE (SIZE(1..maxNumSupQCI)) OF INTEGER | UL Scheduled time per UE per QCI, i.e., total TTIs where that UE was scheduled on the UL for that QCI |
| rank\_dl-1 | SEQUENCE (SIZE(1..maxNumSupQCI)) OF INTEGER | Each element of the array containing the number of Rank 1 samples used by cell for that QCI |
| rank-dl-2 | SEQUENCE (SIZE(1..maxNumSupQCI)) OF INTEGER | Each element of the array containing the number of Rank 2 samples used by cell for that QCI |

**XRANC\_SCHED\_MEAS\_REPORT\_PER\_CELL**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| ecgi | ECGI | Cell ID of associated cell |
| qci\_vals | SEQUENCE (SIZE(1..maxNumSupQCI)) OF QCI | QCI values for which the following information is reported |
| prb-usage-pcell | PRBUsage | Percentage of PRBs used for this ECGI as the primary cell |
| prb-usage-scell | PRBUsage | Percentage of PRBs used for this ECGI as the secondary cell |

**PRBUsage**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| prb\_usage\_dl | SEQUENCE (SIZE(1..maxNumSupQCI)) OF INTEGER(0..100) | (Total number of PRBs allocated over period T in DL/ total number of PRBs \*100) for the reported qci-vals |
| prb\_usage\_ul | SEQUENCE (SIZE(1..maxNumSupQCI)) OF INTEGER(0..100) | (Total number of PRBs allocated over period T in DL/ total number of PRBs \*100) for for the reported qci-vals |

**XRANC\_PDCP\_MEAS\_REPORT\_PER\_UE**

(For definitions see TS 36.314)

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| ecgi | ECGI | Cell ID of associated cell |
| crnti | CRNTI | CRNTI of UE |
| qci\_vals | SEQUENCE (SIZE(1..maxNumSupQCI)) OF QCI | QCI values for which the following information is reported |
| data\_vol\_dl | SEQUENCE (SIZE(1..maxNumSupQCI)) OF INTEGER | PDCP SDU bits delivered from PDCP to RLC per QCI per UE |
| data\_vol\_ul | SEQUENCE (SIZE(1..maxNumSupQCI)) OF INTEGER | PDCP SDU bits received by PDCP at the eNB per QCI per UE |
| pkt\_delay\_dl | SEQUENCE (SIZE(1..maxNumSupQCI)) OF REAL | Average Pkt delay measured from PDCP arrival to MAC exit per QCI per UE |
| pkt\_discard\_rate\_dl | SEQUENCE (SIZE(1..maxNumSupQCI)) OF INTEGER | Average Pkt Discard rate at L2 per QCI per UE |
| pkt\_loss\_rate\_dl | SEQUENCE (SIZE(1..maxNumSupQCI)) OF INTEGER | Average Pkt Loss rate at DL per QCI per UE |
| pkt\_loss\_rate\_ul | SEQUENCE (SIZE(1..maxNumSupQCI)) OF INTEGER | Average Pkt Loss rate at UL per QCI per UE |
| throughput\_dl | SEQUENCE (SIZE(1..maxNumSupQCI)) OF REAL | DL throughput per QCI per UE in kbits/s |
| throughput\_ul | SEQUENCE (SIZE(1..maxNumSupQCI)) OF REAL | UL throughput per QCI per UE in kbit/s |

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| maxNumCQIs | INTEGER ::= 16 | Constant |
| maxNumRIs | INTEGER ::= 2 | Constant |
| sinrHistSize | INTEGER ::= 14 | Constant |
| intrfHistSize | INTEGER ::= 17 | Constant |
| maxNumSupQCI | INTEGER ::= 9 | Constant |

## xICIC/Coordinated Scheduling Controls

**eNodeB**

**xRANc**

**XRANC\_xICIC\_CONFIG**

ICIC Control

Figure 9: ICIC Controls

3.5.1 **XRANC\_xICIC\_CONFIG**

|  |  |  |
| --- | --- | --- |
| Parameters | Type/Value | Description |
| ecgi | ECGI | Cell ID of associated cell |
| crnti | CRNTI | UE identifier |
| pci-arfcn | PCI-ARFCN | PCI and downlink EARFCN of the CC to which the configuration is to be applied |
| p\_a | ENUMERATED (  dB-minus6,  dB-minus4dot77,  dB-minus3,  dB-minus1dot77,  dB-0,  dB-1,  dB-2,  dB-3) | PDSCH power offset for the UE (dB) |
| start\_prb\_dl | INTEGER(0..100) | Starting DL PRB allocated to UE. Valid Range 0 to 100 |
| end\_prb\_dl | INTEGER(0..100) | Ending DL PRB allocated to UE. Valid Range 0 to 100 |
| sub\_frame\_bitmask\_dl | BIT STRING (SIZE(10)) | DL ABS pattern – bitmask. Each bit corresponds to a sub-frame. 0 indicates SF to be allocated to the UE.  LSB corresponds to SubFrame0 |
| p0\_ue\_pusch | INTEGER(-8..7) | PUSCH power offset for the UE (dB). Valid Range [-8, 7] |
| start\_prb\_ul | INTEGER(0..100) | Starting UL PRB allocated to UE. Valid Range 0 to 100 |
| end\_prb\_ul | INTEGER(0..100) | Ending UL PRB allocated to UE. Valid Range 0 to 100 |
| sub\_frame\_bitmask\_ul | BIT STRING (SIZE(10)) | DL ABS pattern – bitmask. Each bit corresponds to a sub-frame. 0 indicates SF to be allocated to the UE.  LSB corresponds to SubFrame0 |

## Carrier Aggregation Controls



Figure 10: Carrier Aggregation Control

**ScellAdd**

|  |  |  |
| --- | --- | --- |
| **Parameters** | **Type/Value** | **Description** |
| **crnti** | CRNTI | C-RNTI of the UE to which the sCell has to be added and activated |
| **ecgi** | ECGI | Cell-Id of the primary cell to which UE is camped on |
| **scells-prop** | SEQUENCE OF PropScell | Properties of the secondary cells to be configured for the UE |

Upon receiving the ScellAdd, eNB sends out RRC connection reconfiguration to the UE with the corresponding scell properties in sCellToAddModList IE. sCell MAC level activation through MAC CE activation is also performed by the Pcell. Upon expiration of deact-timer, the logic of MAC level activation of sCell lies in the eNB scheduler.

**ScellAddStatus**

|  |  |  |
| --- | --- | --- |
| **Parameters** | **Type/Value** | **Description** |
| **crnti** | CRNTI | C-RNTI of the UE to which the sCell are added |
| **ecgi** | ECGI | ECGI of the primary cell of the UE |
| **scells-ind** | SEQUENCE OF PCI-ARFCN | PCI-EARFCN of the secondary cells configured for the UE |
| **status** | SEQUENCE OF ENUMERATED(success, failure) | status of sCell addition |

Sent on RRC reconfiguration complete corresponding to the scell(s) addition.

**ScellDelete**

|  |  |  |
| --- | --- | --- |
| **Parameters** | **Type/Value** | **Description** |
| **crnti** | CRNTI | C-RNTI of the UE to which the sCell has to be deleted |
| **ecgi** | ECGI | ECGI of the primary cell |
| **scells-ind** | SEQUENCE OF PCI-ARFCN | PCI-EARFCN of the secondary cells to be removed for the UE |

Upon getting this message, the eNB sends RRC connection reconfiguration to the UE with the corresponding scell indices in sCellToReleaseList.

**PropScell**

|  |  |  |
| --- | --- | --- |
| **Parameters** | **Type/Value** | **Description** |
| **pci-arfcn** | PCI-ARFCN | PCI-EARFCN of the secondary cell to be configured for the UE |
| **cross-carrier-sched-enable** | BOOLEAN | Cross carrier scheduling is enabled for the UE on this scell |
| **ca-direction** | ENUMERATED (dl, ul, both) | Direction in which CA is enabled |
| **deact-timer** | INTEGER | Value in number of radio frames. SCell deactivation timer in TS 36.321. |